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Boot to proxmox installer tui [image: ]



From ubuntu boot disk:
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Fdisk -l a partir de archiso. Page1:
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journalctl:

Search
invalid option --
:fI5 Jjournalctl

Termina!

-k -b | egrep

Apr 27 15:19:46 ubuntu kernel:

PME il PCIeCapability LTR D

Apr 27 15:19:46 ubuntu kernel:

ubuntu@ubuntu: ~

Help

"
-1
acpi PNPOAO8:00:
PC]

acpi PNPOAO8:02:

_0SC: 0S now controls

_0SC: 0S now controls

'mpt3sas|megaraid|ahci|nvme|reset|timeout|aer’

PCIeHotplug SHPCHotplug|

PCIeHotplug SHPCHotplug|

PME jl PCIeCapability LTR DPC]

Apr 27 15:19:46 ubuntu kernel: acpi PNPOAG8:03:
PME il PCIeCapability LTR DPC]

27 15:19:46 ubuntu kernel: pcieport

27 15:19:46 ubuntu kernel: pcieport

27 15:19:46 ubuntu kernel: pcieport

27 15:19:46 ubuntu kernel: pcieport

27 15:19:46 ubuntu kernel: pcieport

15:19:46 ubuntu kernel: pcieport

27 15:19:46 ubuntu kernel: E—_—

00000dcffcO00 mapped virt_addr:Ox(___ |

15:19: ubuntu kernel: NEEEESEE sas

15:19: ubuntu kernel: NN S35

_0SC: 0S now controls [PCIeHotplug SHPCHotplug|
0000:
0000:
0000:

0000:

00:
00:
00:

01.
03.
11.
ic.

N B
N B
N B
N B
0000: 1c.4: JEN:
0000:00:1c.7: N:
sas 0000:01: GO 0:
ptrval___ )
0000:01:00.
0000:01:00.

enabled
enabled
enabled
enabled
enabled
enabled
BAR:0x1

26
27
28
29

with
with
with
with
with IRQ 30

with IRQ 31

BAR's base_addr(phys):0x000|

IRQ
IRQ
IRQ
IRQ

46
46

: FW now in Ready state
: 63 bit DMA mask and 32 bit consisten

15:19:46 ubuntu kernel: [N s3s 0000:01:00. requested/available msix 1/1 poll_qu

15:19:46 ubuntu kernel: [ S2s 0000:01:00.0: current msix/max num queues

IApr 27 15:19:46 ubuntu kernel: [N sas 0000:01:00.0: RDPQ mode (disabled)

IApr 27 15:19:46 ubuntu kernel: [l 0000:00:1f.2: | vers 0001.0300, 32 command slots, 3 Gbp|
s, SATA mode

JApr 27 15:19:46 ubuntu kernel: | 0000:00:1f.2: 5/6 ports implemented (port mask Ox1f)

IApr 27 15:19:46 ubuntu kernel: [l 0000:00:1f.2: flags: 64bit ncq sntf pm led clo pio slum pga|
rt ems apst

Apr 27 15:19:46 ubuntu kernel: scsi hostl:
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Search Terminal

27
27
27
27
27
27
27
Apr 27
Enabled
27 15:
27 15:1
27 15:

Apr
Apr
Apr
Apr
Apr

27 15:

58

9:46
9:46
9:46

9:46

ubuntu
ubuntu
ubuntu
ubuntu
ubuntu
ubuntu
ubuntu
ubuntu

ubuntu
ubuntu
ubuntu

: 0 secs/0O secs
19:46 ubuntu

ubuntu

Help

kernel: scsi hostl: [N
kernel: scsi host2: [
kernel: scsi host3: [
kernel: scsi host4: [
kernel: scsi host5: [
kernel: scsi host6: [
kernel: [N sas 0000:01:00.
kernel: | sas 0000:01:00.
kernel: [N sas 0000:01:00.
kernel: NN sas 0000:01:00.
kernel: NN sas 0000:01:00.
kernel: NN saos 0000:01:00.

kernel:

15:

15:

9:46

19:46 ubuntu

ubuntu

15:19:46 ubuntu

kerne

kernel:
kerne

Apr 27 15:1
9

Apr 27 15:1
Apr 27 15:1
list failed
Apr 27 15:1
Apr 27 15:

9:46

9:46
9:46

9:46
50

ubuntu

ubuntu
ubuntu

ubuntu
ubuntu

kernel:

kernel: SN sas 0000:01:00.
kernel: NN sas 0000:01:00.
kernel: [ sas oood:01:00.
kernel: power meter ACPIOOOD:00:

| EEB
: O sas

| KB
: I sas

| KB

ubuntu@ubuntu: ~

0000:01:

0000:01:

0000:
0000:

01:
01:

0000:01:

: controller type
: Online Controller |M(OCR)

: I passthru support

00.
00.0: megasas_init_mfi:

00.
00.
00.

: megasas_init_fw:

Naltlng for ACPI IPMI EEEEE

iMR(OMB)

: No
No
FW provided TM TaskAbort/Reset timeo

Secure JBOD support

JBOD sequence map support H

PCI Lane Margining support

fw_support_ieee=67|

INIT adapter done
JBOD sequence map is disabled megasa

Failed from megasas_issue_polled 112

failed to get LD list
megasas_get_device

Failed from megasas_init_fw 6553
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ubuntu@ubuntu:-$ Lspcit -k -s 01:00.0

01:00.0 RAID bus controller: Broadcom / LSI MegaRAID SAS 2008 [Falcon] (rev 03)
DeviceName: Integrated RAID
Subsystem: Dell PERC H310 Mini Monolithics
Kernel modules: megaraid_sas
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File Edit View Search Terminal Help
dmesg: read kernel buffer failed: Operation not permitted
uguntu@ubuntu:-$ sudo dmesg -T | egrep -1 'ahci|ata|SATA link'
[Mon, Apr 27 15:16:18 2026] BI0OS-e820: [mem 0x00000000b89c4000-0x00000000b8a43fff] ACPI d-
[Mor® Apr 27 15:16:18 2026] BIOS-e820: [mem 0x00000000bd31c000-0x00000000bd35afff] ACPI d- -
o [Mon Apr 27 15:16:18 2026] NODE_D' ' '(0) allocated [mem 0x183ffd52c0-0Ox183fffffff]
[Mon Apr 27 15:16:18 2026] printk: log buffer d-'> + meta d-"-: 262144 + 917504 = 1179648 byte

s
[Mon Apr 27 15:16:19 2026] Memory: 98693104K/100598572K available (22209K kernel code, 4649K r
wd-©, 16288K rod- -, 5264K init, 4216K bss, 1886528K reserved, 0K cma-reserved)

[Mon Apr 27 15:16:19 2026] lib- - version 3.00 loaded.

[Mon Apr 27 15:16:19 2026] Write protecting the kernel read-only d-=-: 38912k

[Mon Apr 27 15:16:19 2026] Freeing unused kernel image (text/rod - gap) memory: 316K

[Mon Apr 27 15:16:19 2026] Freeing unused kernel image (rod- -/d- - gap) memory: 96K

[Mon Apr 27 15:16:20 2026] usb 1-1.2: Product: D--Traveler 2.0

[Mon Apr 27 15:16:20 2026] usb 2-1.2: Product: D-"-Traveler 3.0

[Mon Apr 27 15:16:20 2026] -~ 0000:00:1f.2: " vers 0001.0300, 32 command slots, 3 Cbps, S
474 mode

[Mon Apr 27 15:16:20 2026] -~ 0000:00:1f.2: 5/6 ports implemented (port mask Ox1if)

[Mon Apr 27 15:16:20 2026] -~ 0000:00:1f.2: flags: 64bit ncq sntf pm led clo pio slum part e
ms apst

[Mon Apr 27 15:16:20 2026] scsi hostl: -

[Mon Apr 27 15:16:20 2026] scsi host2: i@

[Mon Apr 27 15:16:20 2026] scsi host3: i@

[Mon Apr 27 15:16:20 2026] scsi hostd4: -1

[Mon Apr 27 15:16:20 2026] scsi host5: ~hct

[Mon Apr 27 15:16:20 2026] scsi host6: i@

[Mon Apr 27 15:16:20 2026] -~ ~1: S' ~ max UDMA/133 abar m2048@0xdfeffeee port Oxdfoff1ee irqg 3
~e 4 lpm-pol 1 ext fﬁg:f‘
.\., [Mon Apr 27 15:16:20 2026] -~ -2: S' ~ max UDMA/133 abar m2048@0xdfeffeee port exdfeff180 irq 3

A 1nm-nal 1 avt
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4 1pm-pol 1 ext

[Mon Apr 27 15:16:20 2026] - -2: S' ' max UDMA/133 abar m2048@0xdfeffee0 port Oxdfoff180 irq 3
4 1pm-pol 1 ext

[Mon Apr 27 15:16:20 2026] - =3: S' " max UDMA/133 abar m2048@0xdfeffee0 port Oxdfoff200 irq 3
4 lpm-pol 1 ext

[Mon Apr 27 15:16:20 2026] - -4: S' ' max UDMA/133 abar m2048@0xdfoffeee port Oxdfeff280 irq 3
4 lpm-pol 1 ext

[Mon Apr 27 15:16:20 2026] - -5: S' ' max UDMA/133 abar m2048@0xdfoffeee port Oxdfeff3ee irq 3
4 1pm-pol 4

[Mon Apr 27 15:16:20 2026] - -6: DUMMY

[Mon Apr 27 15:16:20 2026] - =4: " . down (SStatus © SControl 300)

[Mon Apr 27 15:16:20 2026] - =2: -~~~ . down (SStatus @ SControl 300)

[Mon Apr 27 15:16:20 2026] -~ =5: “~  _n: up 1.5 Gbps (SStatus 113 SControl 300)

[Mon Apr 27 15:16:20 2026] - =1: " " down (SStatus © SControl 300)

[Mon Apr 27 15:16:20 2026] - =3: " . down (SStatus @ SControl 300)

[Mon Apr 27 15:16:20 2026] - -5.00: " '/PI: PLDS DVD-ROM DS-8D9SH, UD51, max UDMA/100

[Mon Apr 27 15:16:20 2026] - -5.00: configured for UDMA/100

S Bl aON |

[Mon Apr 27 15:16:21 2026] scsi 8:0:0:0: Direct-Access Kingston D~ -Traveler 3.0 0000 PQ:
O ANSI: 4

[Mon Apr 27 15:16:21 2026] scsi 7:0:0:0: Direct-Access Kingston D~ -Traveler 2.0 PMAP PQ:
O ANSI: 0 CCS

[Mon Apr 27 15:19:46 2026] systemd[1]: systemd-hwdb-update.service - Rebuild Hardware D ' - base
was skipped because no trigger condition checks were met.

[Mon Apr 27 15:19:52 2026] ZFS: Using ZFS with kernel 6.17.0-14-generic is EXPERIMENTAL and SE
RIOUS D" " LOSS may occur!

[Mon Apr 27 17:52:55 2026] -=-1: “° . down (SStatus @ SControl 300)

[Mon Apr 27 17:54:25 2026] -~ -1: ~° 1 down (SStatus @ SControl 300) 1
~e [Mon Apr 27 17:54:25 2026] =t:2: A7/ Link down (SStatus @ SControl 300) )
i\.) [Mon Apr 27 17:54:25 2026] - =3: /1. lmtatus © SControl 300) I

[Mon Apr 27 17:54:26 20261 -~ 4: ' ' < tatus O SControl 300)
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[Mon Apr 27 15:16:20 2026] - =3: S' ' max UDMA/133 abar m2048@0xdfoffeee port Oxdfeff200 irq 3
4 lpm-pol 1 ext
[Mon Apr 27 15:16:20 2026] -~ -4: S' ' max UDMA/133 abar m2048@0xdfeffee0 port Oxdfoff280 irq 3
4 1pm-pol 1 ext
[Mon Apr 27 15:16:20 2026] - -5: S' ' max UDMA/133 abar m2048@0xdfoffee0 port Oxdfoff3e0 irq 3
4 1pm-pol 4
[Mon Apr 27 15:16:20 2026] - =6: DUMMY
[Mon Apr 27 15:16:20 2026] - -4: ~~° . down (SStatus © SControl 300)
[Mon Apr 27 15:16:20 2026] -~ =2: ~~ ~ " down (SStatus @ SControl 300)
[Mon Apr 27 15:16:20 2026] - ==5: “~  _n: up 1.5 Gbps (SStatus 113 SControl 300)
[Mon Apr 27 15:16:20 2026] - =1: "~ . down (SStatus © SControl 300)
[Mon Apr 27 15:16:20 2026] - =3: ~~ . down (SStatus @ SControl 300)
[Mon Apr 27 15:16:20 2026] -::5.00: /' 'PI: PLDS DVD-ROM DS-8D9SH, UD51, max UDMA/160
[Mon Apr 27 15:16:20 2026] - -5.00: configured for UDMA/100
[Mon Apr 27 15:16:21 2026] scsi 8:0:0:0: Direct-Access Kingston D~ -Traveler 3.0 0000 PQ:
O ANSI: 4
[Mon Apr 27 15:16:21 2026] scsi 7:0:0:0: Direct-Access Kingston D~ -Traveler 2.0 PMAP PQ:
O ANSI: 0 CCS
[Mon Apr 27 15:19:46 2026] systemd[1]: systemd-hwdb-update.service - Rebuild Hardware D~ base
was skipped because no trigger condition checks were met.
[Mon Apr 27 15:19:52 2026] ZFS: Using ZFS with kernel 6.17.0-14-generic is EXPERIMENTAL and SE
RIOUS D'~ LOSS may occur!
[Mon Apr 27 17:52:55 2026] - -1: “~ ~ . down (SStatus @ SControl 300)
[Mon Apr 27 17:54:25 2026] - -1: " . down (SStatus © SControl 300)
]
]

. = i @
4

[Mon Apr 27 17:54:25 2026] ~:-2: “~'/ .o down (SStatus © SControl 300)
[Mon Apr 27 17:54:25 2026] - =-3: /" . down (SStatus @ SControl 300)
[Mon Apr 27 17:54:26 2026] -~ -4: ~° 1 down (SStatus @ SControl 300)
[Mon Apr 27 17:54:26 2026] - =5: “° © _n: up 1.5 Gbps (SStatus 113 SControl 300)

[Mon Apr 27 17:54:26 2026] -:25.00: confwmwlee {@CT
ubuntu@ubuntu:-¢ B

Activer'

L]
o
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n Ux0bl FIE Kead access 1s not set

[ 148.0811811 DMAR: DRHD: handling fault status reg 2

[ 148.0818481 DMAR: [DMA Read NO_PASID] Request device [01:00.0] fault addr Oxbd43c000 [fault reaso
n 0x061 PTE Read access is not set

[ 148.0934681 DMAR: DRHD: handling fault status reg 102

[ 148.0941461 DMAR: [DMA Read NO_PASID] Request device [01:00.0] fault addr O0xbd43c000 [fault reaso
n 0x061 PTE Read access is not set

Begin: Running /scripts/local-block ... done.
[ 148.105757]1 DMAR: DRHD: handling fault status reg 202
Begin: Running /scripts/local-block ... done.
Begin: Running /scripts/local-block ... done.
Begin: Running /scripts/local-block ... done.
Begin: Rumming sscripts/local-block ... done.

[ 153.0799991 dmar_fault: 1160 callbacks suppressed
[ 153.0800091 DMAR: DRHD: handling fault status reg 502

153.0824121 DMAR: [DHMA Read NO_PASID] Request device [01:00.0] fault addr 0xbd43c000 [fault reaso
0x061 PTE Read access is not set

153.096000]1 DMAR: DRHD: handling fault status reg 602

153.0966951 DMAR: [DMA Read NO_PASID] Request device [01:00.0] fault addr Oxbd43c000 [fault reaso
0x061 PTE Read access is not set

153.1082091 DMAR: DRHD: handling fault status reg 702

153.1089061 DMAR: [DMA Read NO_PASID] Request device [01:00.0]1 fault addr Oxbd43c000 [fault reaso
0x061 PTE Read access is not set

153.1204951 DMAR: DRHD: handling fault status reg 2
Begin: Running /scripts/local-block ... done.
done.
Gave up waiting for root file system device. Common problems:

- Boot args (cat /procscmdline)

- Check rootdelay= (did the system wait long enough?)

- Missing modules (cat /proc/modules: ls sdev)
ALERT! ,/deu/mapper/pue-root does not exist. Dropping to a shell?

ek Rakal Nl

-z

BusyBox v1.35.0 (Debian 1:1.35.0-4+b?) built-in shell (ash) ) _
Enter "help’ for a list of built-in commands. Activer Wind

Accédez aux para
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Disk /dev/sda: 1.82 Tib, 1933844147200 bytes, 3905945600 sectors
Disk model: PERC H310

Units: sectors of 1 = 512 = 512 bytes

Sector size (logical/physical): S12 bytes / S12 bytes

10 size (wininun/optinal): 512 bytehy/ 512 bytes

Disklabel type: gpt

Disk identifier: 2176A016-7EGF-4292-B19-BC01026CIFA

Device Start End  Sectors Size Type
devssdal 3 2047 2014 1007k BIOS boot
Aev/sidaz 2048 2099199 2097152 1G EFI Systen

Adewssdad 2099200 209715200 207616001 996 Limux LUK
sdevssdad 209717248 1256293247 1048576000 5006 Limux LUK
AevssdaS 1256293248 2306869247 1048576000 5006 Limux filesysten

Disk /de/sdc: 57.73 GiB, 61991813632 bytes, 121077761 sectors
Disk model: DataTraveler 3.0

Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

140 size (mininun/optinal): 512 bytes / 512 bytes

Disklabel type: dos

Disk identifier: 0x0093dde1

Device  Boot Start End  Sectors Size 1d Type
Aevssdcl w2048 121077695 121075648 57.76 c UIS FATIZ (LBA)

Disk /deu/loopd: 973.08 MiB, 1020346368 bytes, 1992864 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

140 size (minimumoptimal): 512 bytes / 512 bytes

Disk /dev/mapper/pue-suap: B GiB, BSBI9HMSI2 bytes, 16777216 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (ninimun/optinal): 512 bytes / 512 bytes

Disk /dev/mapper/pue-root: 34.75 Gib, 37308334080 bytes, 72867640 sectors
Units: sectors of 1 » 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (nininun/optinal): 512 bytes / 512 bytes

Disk /deu/mapper/pue-un-—102--disk—0: 23 GiB, 24696061952 bytes, 4B2344% sectors
Units: sectors of 1 « 512 = 512 bytes

Sectar size (logical/physical): 512 bytes / 512 bytes

10 size (minimun/optinal): 6553 bytes / 65536 bytes

Disk /deu/mapper/pue-un--103--disk--0: 30
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes
10 size (minimun/optinal): 6553 bytes / 65536 bytes

32212254720 bytes, 62914560 sectors

Disk /deu/mapper/pue-un--105--disk--0: 30 GiB, 32212254720 bytes, 62914560 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

140 size (wininun/optinal): 65536 bytes / 6553 bytes
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sdevssdel = 2048 121077695 121075648 57.76 c W95 FAT3Z (LBA)

Disk /dev/loopd: 973.08 MiB, 1020346368 bytes, 1992864 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (minimun/optinal): 512 bytes / 512 bytes

Disk /deu/mapper/pue-suap: B Gil, 8589934592 bytes, 16777216 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (minimunoptinal): 512 bytes / 512 bytes

Disk deu/mapper/pue-root: 34.75 Gib, 37308334080 bytes, 72867640 sectors
Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (ninimun/optinal): 512 bytes / 512 bytes

Disk /deu/mapper./pue-un--102-—disk—0: 23 GiB, 24696061952 butes, 462344% sectors
Units: sectors of 1 = 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (nininun/optinal): 65536 butes / 6553 bytes

Disk /dev/mapper/pue-un-—-103--disk—0: 30 GiB, 32212254720 bytes, 62914560 sectors
Units: sectors of 1 = 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (minimun/optinal): 6553 bytes / 65536 butes

Disk /dev/mapper/pue-un--105--disk--0: 30 GiB, 32212254720 bytes, 62914560 scctars
Units: sectors of 1 » 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

140 size (minimun/optinal): 6553 bytes / 65536 bytes

Disk /deu/sdb: 1.82 Tib, 2000365289472 bytes, 3906963456 sectors
Disk model: My Book 1230

Units: sectors of 1 = 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (nininun/optinl): 512 bytes / 512 bytes

Disklabel tupe: dos

Disk identifier: 6x792b8081

Device  Boot Start End  Sectors Size 1d Type
deussdbl 2048 3996363455 390691408 1.8T 7 HPFSNTFS/exFAT

Disk /dev/sdf: 57.73 Gib, 61991613632 bytes, 121077761 sectors
Disk model: DataTraveler 3.0

Units: sectors of 1 % 512 = 512 bytes

Sector size (logical/physical): 512 bytes / 512 bytes

10 size (ninimun/optinal): 512 bytes / 512 bytes

Disklabel type: gpt

Disk identifier: BI0B3023-1E94-45DC-ABA3-DAGBBEOININ)

Device Start  End Sectors Size Type
Alewssify 64 635 572 286K Microsoft basic data
sdevssdf2 636 12619 16384 BN EFI Systen

dev/sdf3 17620 3577255 3560236 1.76 Apple HFSAIFS+
sdev/sdfd 3577256 3572855 600 300K Microsoft basic data
rootéarchiso ~ #




image1.png
Warning: Attach Partition IPMI command failed. Retrying for 6 times...
Initializing firmware interfaces...
Initialization complete.
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Timed out for waitinghthe udeuv queue being empty.
Timed out for waiting the udev queue being empty.
Gave up waiting for root file system device. Common problens:
- Boot args (cat /procscmdline)
— Check rootdelay= (did the system wait long enough?)
- Missing modules (cat /proc/modules: Is sdeuv)
ALERT! sdeus/mapper/pue-root does not exist. Dropping to a shellt

BusyBox v1.35.0 (Debian 1:1.35.0-4+b?) built-in shell (ash)
Enter "help’ for a list of built-in commands.

(initramfs) _
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GNU GRUB wersion 2.06-13+pmx6

etparams 'Proxmox YE GNU-SLinux'

load_video

insmod €zio

if [ =®grub_platform = xxen ]; then insmod xzio; insmod lzopio; fi
insmod part_gpt

insmod lwvm

insmod ext2

set root='lvmid/vnukAH-AYxe-stvD-EFQC-B2V2-fVGU-NegyYcd /WEGLNG -h430-eMRH-wCno-qgveyY-pMy

[ x$feature_platform_search_hint = xy 1; then
search --no-floppy --fs-uuid --set=root --hint='lvmid/VnuwkAH-AYxe-stv0-EFQC-B2V2-fN
VGU-NegYcd /wEOLNG -hd430-eMRH-wCne-gveyY-pMye-5CeMxa’ bdSees2d-eb29-43a0-8f6e-0Sefagefaebl

else

search --no-floppy --fs-uulid --set=root bdS6e32d-oh29-43a0-8fce-0Sefadefaebl
fi
echo 'Loading Linux 6.8.12-9-pve ...
linux /bootsvmlinuz-6.8.12-9-pve root=sdev/mapper/spve-root ro gquiet
echo 'Loading initial ramdisk ...'
initrd sbootsinitrd. img-6.8.12-9-pve

Minimum Emacs-1like screen editing is supported. TAB lists completions. Press Ctrl-x
or F1o to boot, Ctrl-c or F2 for a command-line or ESC to discard edits and return

A . 8 .  emrma aEm
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Loading Linux 6.8.12-9-pve ...

Loading initial ramdisk ...
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.1019781
.1036001
.1050961
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.2846561
.2855041
.2874981
.2882951
.2890941
.2899291
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7506881
2907051
2907171
.2935551

NN UT A D WD D DD

S

LRL:
@ o™ ¢
I-X-X-%
I-R-R-¥
-X-R-%

S

Bk~ bl }

: [sdbl 121077761 S12-byte logical blocks: (62.0 GB/57.7 GiB)
: [sdb] Urite Protect is off
: [sdb]l Write cache: disabled, read cache: enabled, doesn’t support DPO or

GPT:Primary header thinks Alt. header is not at the end of the disk.

GPT:3070107 t= 121077760

GPT:Alternate GPT header not at the end of the disk.

GPT:3070107 = 121077760

GPT: Use GNU Parted to correct GPT errors.

sdb: sdbl sdbZ sdb3 sdb4

sd 8:0:0:0: [sdb] Attached SCSI removable disk

randon: crng init done

dmar_fault: 6?62 callbacks suppressed

DMAR: DRHD: handling fault status
DMAR: [DMA Read NO_PASID] Request

0x06]1 PTE Read access is not set

7.3029291
7.3049421

DMAR: DRHD: handling fault status
DMAR: [DMA Read NO_PASID] Request

0x061 PTE Read access is not set

7.3152171
7.3122091

DMAR: DRHD: handling fault status
DMAR: [DMA Read NO_PASID] Request

0x061 PTE Read access is not set

7.3275041

DMAR: DRHD: handling fault status

reg 402
device [01:00.0]

reg 502
device [01:00.0]

reg 602
device [01:00.0]

reg 702

12.2980651 dmar_fault: 1111 callbacks suppressed
12.2980741 DMAR: DRHD: handling fault status reg 702

12.3008111

DMAR: [DMA Read NO_PASID] Request

0x061 PTE Read access is not set

12.3102781
12.3122261

DMAR: DRHD: handling fault status
DMAR: [DMA Read NO_PASID] Request

0x061 PTE Read access is not set
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12.3245411

DMAR: DRHD: handling fault status
DMAR: [DMA Read NO_PASID] Request

0x061 PTE Read access is not set

12.3348541

DMAR: DRHD: handling fault status
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fault

fault

fault

fault

fault

fault

addr

addr

addr

addr

addr

addr

0xbd43c000

0xbd43c000

0xbd43c000

0xbd43c000

0xbd43c000

0xbd43c000

[fault

[fault

[fault

[fault

[fault

[fault

reaso

reaso

reaso

reaso

reaso

reaso
Activer Windo

Accédez aux paranm




image6.png
0.934421] Initranfs unpacking failed: ZSTD-compressed data is corrupt




